       Release Notes for Version 17.07.02 of the J1699-3 software


Except for the issues detailed in 'J1633-3 Work Status', this release includes the
requirements of revision 17.7 of the J1699-3 document and is intended to
test Model Year 2025 and beyond, that are compliant with SAE J1979.



NOTES:
 - This release only supports the 0404 version of the J2534 API!
 - Slow PCs/J2534 devices may cause false vehicle failures!
 - J2534 Interfaces that do not support all of the protocols being tested will result in the vehicle failing J1699-3.
 - To avoid false failures during the CARB Drive Cycle, do NOT operate the vehicle at exactly 25 MPH (40KPH).
 - For EOBD ONLY, scanning CAN baud rates may cause ECUs to go BUS_OFF!
 - The file "J1699 User Notes.doc" is a simple User Guide to the J1699-3 software.
 
!!!!NEW NOTE!!!!
 - Command Prompt for Window must be at least 33 rows tall
   Windows 10 and earlier: Right click Command Prompt Title Bar, Left click Properties, Left click Layout Tab, Set Window Size Height to at least 33 (Screen Buffer Size Height should be significantly larger).
   Windows 11: Right click Command Prompt Title Bar, Left click Settings, Scroll Down to Launch Size, On the right-hand side, Left click Drop Down Menu Arrow, Set Rows to at least 33.


Version 17.07.02 adds the following features:
Issue #     Description

Version 17.07.02 fixes the following issues:
Issue #     Description
1083        fix Data D bit 4 falsely failing gasoline vehicles.
